Selected Tables          	Release 62    	Last Change 04apr26 12:01
Original RBIL Copyright (c) 1989-1999,2000 Ralf Brown
Modifications Copyright (c) 2026 The List Project and its contributors
--------!---TABLES---------------------------
Buses
	EISA (see INT 15/AX=D800h)
	I2C / IIC bus (see I2C 00h)
	PCI bus -- see below
	System Management Bus (see INT 15/AX=53B0h/BH=01h)
	Universal Serial Bus OpenHCI (see #00902 at INT 1A/AX=B10Ah)

Country-Specific Information:
	country codes (see #01400 at INT 21/AH=38h)
	country-specific information (see #01398,#01399)
	country-dependent capitalization (see INT 21/AX=6520h)
	code pages (see #00470,#01757)
	extended country-specific info (see #01750 at INT 21/AX=6500h)
		uppercase table (see #01751)
		filename uppercase table (see #01753)
		filename terminator table (see #01754)
		collating table (see #01755)
		DBCS lead byte table (see #01756)
	yes/no response (see INT 21/AX=6523h)

DESQview
	.PIF / .DVP file format (see #00427 at INT 15/AX=102Ch)
	TopView panel file format (see #00436 at INT 15/AH=12h)
	TopView/DESQview streams (see #00446,#00447,#00448 at INT 15/AH=12h)

DOS (general)
	DOS commandline (see #02585 at INT 2E)
	DOS Environment block (see #01378 at INT 21/AH=26h,#01395)
	DOS memory allocation strategy (see #01679 at INT 21/AH=58h)
	DOS OEM number (see #01394 at INT 21/AH=30h)

DOS EXEC function (see INT 21/AH=4Bh):
	EXEC parameter block (see #01590,#01591,#01592)
	.EXE file formats (see #01594,#01596,#01609,#01616)
	Program Segment Prefix (PSP) (see #01378 at INT 21/AH=26h)

DOS error codes (see INT 21/AH=59h)
	critical error (see #02545 at INT 24)
	extended error codes (see #01680)
	error class (see #01682)
	error locus (see #01684)
	media ID structure (see #01681)
	recommended action (see #01683)

DOS extenders
	DPMI error codes (see #03143 at INT 21/AX=0000h)
	DPMI mode switch (see #02718 at INT 2F/AX=1687h)
	DPMI vendor-specific API (see #02719 at INT 2F/AX=168Ah)
	DPMS registration structure (see #02793 at INT 2F/AX=43E0h)
	VCPI (see INT 67/AX=DE00h)
		mode switch (see #03665 at INT 67/AX=DE0Ch)

DOS-internal data (see INT 21/AH=52h)
	Current Directory Structure (see #01643,#01644,#01645)
	Disk buffer (see #01649,#01650,#01652,#01653,#01655)
	DOS Parameter List (DPL) (see #01686 at INT 21/AX=5D00h)
	IFS entry point (see #01658)
	List of Lists (SYSVARS) (see #01627)
	Memory Control Block (see #01628,#01630,#01633)
	Novell DOS (see #01584,#01585 at INT 21/AX=4458h)
	SHARE hooks (see #01636)
	Swappable Data Area (SDA) (see #01687,#01690 at INT 21/AX=5D0Bh)
	System File Table (SFT) (see #01639,#01640,#01641,#01642)

Device Drivers
	command code (see #02595 at INT 2F/AX=0802h)
	device driver header (see #01646 at INT 21/AH=52h)
	device attributes (see #01647,#01648 at INT 21/AH=52h)
	error codes (see #02598 at INT 2F/AX=0802h)
	request header (see #02596 at INT 2F/AX=0802h)

Disks
	BIOS Parameter Block (BPB) (see #01663)
	diskette drive type (see #00242 at INT 13/AH=08h)
	diskette parameter table (see #01264 at INT 1E)
	DOS drive parameter block (see #01357 at INT 21/AH=1Fh)
	DOS media ID byte (see #01356 at INT 21/AH=1Bh)
	hard disk master boot sector (see #00650 at INT 19)
	hard disk partition record (see #00651 at INT 19)
	IDE controller commands (see #P0515 at PORT 01F0h)
	Partition Types (see #00652 at INT 19)
	serial number (see #01565 at INT 21/AX=440Dh,#01766 at INT 21/AH=69h)

Error Codes (Other)
	AMI/Award/C&T/etc. BIOS diagnostics (POST) codes (see #P0410,#P0412)
	Advanced Power Management [APM] (see #00473 at INT 15/AX=5300h)
	EMS (see #03648 at INT 67/AH=40h)
	PRINT.EXE (see #02594 at INT 2F/AX=0101h)
	XMS (see #02775 at INT 2F/AX=4310h)

Files and Directories
	Directory Entry: MS-DOS, DR DOS, Novell DOS (see #01352)
	file attributes (see #01401 at INT 21/AH=3Ch)
	File Control Block (FCB) (see #01345 at INT 21/AH=0Fh)
	File Date and Time (see #01665,#01666 at INT 21/AX=5700h)
	file-sharing behavior (see #01403 at INT 21/AH=3Dh)
	FindFirst data block (see #01626 at INT 21/AH=4Eh)
	Long File Names (see INT 21/AH=71h,#01355 at INT 21/AH=11h)

Keyboard
	keyboard controller commands (see #P0386,#P0401)
	scan codes (see #00006 at INT 09"IRQ1")
	shift states (see #00587,#00588 at INT 16/AH=12h)

Memory
	memory size (see INT 12,INT 15/AH=88h,INT 15/AX=E820h)
	SDRAM/DIMM configuration data (see #I0047 at I2C A0h)

NetWare
	DOS Requester entry point (see #02859 at INT 2F/AX=7A20h)
	error codes (see #01807 at INT 21/AH=BCh,#01811,#01834 at INT 21/AH=E1h)
	LSL status (see #02989 at INT 2F/AX=C000h"LSL")
	NetWare Core Protocol functions (see #02095 at INT 21/AH=F2h)
	VLM error codes (see #02860 at INT 2F/AX=7A20h)
	VLM header (see #02862 at INT 2F/AX=7A20h)
	VLM identifier (see #02861 at INT 2F/AX=7A20h)

Other Tables
	AMIS signatures (see #02569,#02570 at INT 2D/AH=00h)
	BIOS equipment list (see #00226 at INT 11)
	BIOS32 Service Directory (see #F0021)
	Interrupt Sharing Protocol (ISP) header (see #02568 at INT 2D)
	Multiprocessor Specification - Floating Pointer Structure (see #M0113)
	Option ROM header (see #F0082)
	ROM configuration table (see #00509 at INT 15/AH=C0h)

PCI Bus
	PCI BIOS error codes (see #00729 at INT 1A/AX=B101h)
	PCI configuration data (see #00878 at INT 1A/AX=B10Ah)
	PCI vendor ID (see #00732 at INT 1A/AX=B102h)
	PCI IRQ Routing Table (see #01259 at INT 1A/AX=B406h)

Plug-and-Play
	Plug-and-Play Installation Structure (see #F0024)
	Plug-and-Play error codes (see #F0081)
	Plug-and-Play device type codes (see #F0085)
	Extended System Configuration Data (ESCD)(see #01244 at INT 1A/AX=B401h)
	generic device IDs (see #F0086)

Power Management
	Advanced Power Management [APM] (see INT 15/AX=5300h)
	Advanced Configuration and Power Interface [ACPI]
		(see #M0094 at MEM xxxxh:xxx0h"ACPI")

Real-Time Clock (see also CMOS.LST)
	status registers (see #00406,#00407,#00408 at INT 15/AH=01h"Amstrad")

Serial Port
	serial port parameters (see #00300 at INT 14/AH=00h)
	serial line status (see #00304 at INT 14/AH=03h)
	modem status (see #00305 at INT 14/AH=03h)

Sound
	Adlib/SoundBlaster registers (see #P0645 at PORT 0388h"AdLib")
	Gravis UltraSound
		registers (see #P0593 at PORT 0340h"Gravis")
		board version (see PORT 0746h"Gravis")
		MegaEm (see INT 21/AX=FD12h,#03975 at INT 81/AX=0200h)
	SoundBlaster SBSIM (see #03972 at INT 80"SBSIM")
	Windows Sound System (see #P0895 at PORT 0530h"Windows Sound")

Video
	character attributes (see #00014 at INT 10/AH=08h)
	Display Combination Code (DCC) (see #00039 at INT 10/AX=1A00h)
	TopView/RSIS shadow buffer [virtual screen] (see INT 10/AH=FEh)
	VESA DDC monitor information (see #00127 at INT 10/AX=4F15h/BL=01h)
	VESA SuperVGA information (see #00077 at INT 10/AX=4F00h)
	video modes
		mode numbers (see #00010 at INT 10/AH=00h)
		UltraVision modes (see #00220 at INT 10/AX=CD04h)
		VESA modes (see #00083 at INT 10/AX=4F02h)
	video parameters (see #01263 at INT 1D)

Windows
	Global EMM Import record (see #01515 at INT 21/AX=4402h)
	Startup Information Structure (see #02631 at INT 2F/AX=1605h)
	VMMCALL (see INT 20"Windows")
	VxD identifiers (see #02642 at INT 2F/AX=1684h)
--------!---CONTACT_INFO---------------------
The List Project is in not affiliated with Ralf Brown or his original
Interrupt List, which he maintained up to July 2000 as the Release 61.
We are very grateful for his efforts and intend to continue improving and
adding to that work as The List Project. All contact to The List Project
should be performed through GitHub at: https://github.com/LoopZ/TheList

To find a copy of the original Ralf Brown's Interrupt List or to contact him,
please visit his webpage at http://www.cs.cmu.edu/~ralf/
